AEG Olympia ESW 2000 - Alternate Dip Switch S

DocumentID: 600835
Revision Date: 29-Feb-96 1:28:31 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer using an AEG Olympia ESW 2000 printer received a blank sheet of paper after each printed page. The dip switches were set to the recommended setting of 7 and 9 On and all others Off. Changing the switch settings to 4, 5, 7 and 9 On and all of the rest Off solved the problem.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.