HP LaserJet III - Adjusting Redline Shading

DocumentID: 637201
Revision Date: 29-Feb-96 3:04:32 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The following are instructions for adjusting the Redline shade on any HP LaserJet III type printer on any release date of the printer driver: 1. Retrieve the WPHP1.ALL file into the PTR Program, and press Enter on the HP LaserJet III printer. 2. Cursor to Attribute methods, and press Enter. 3. Cursor to Redline, and press Enter twice. 4. Cursor to Redline Off, and press Enter. The variable name listed here will be the variable you will need to edit (e.g., hp3redoff). If none is listed, skip to step 7. 5. Press Alt-F8 (Global variables). 6. Cursor to the variable, and press Ctrl-Enter. 7. You should see a string that reads ...15g2P". Edit the 15 to a smaller number, e.g. ...10g2P". The number represents the shade percentage. If you do not see this string listed anywhere in the command lines, see if another variable is listed (e.g., hpredoff). Exit back to the global string list, and repeat steps 6 and 7. 8. Exit, save, and replace the file. Then update the .PRS file in WP (Shift-F7, S, U).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.