Fixed Frequency Monitor

DocumentID: 644437
Revision Date: 29-Feb-96 8:18:59 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A fixed frequency monitor is an analog monitor that operates using a fixed horizontal sync frequency. Vertical sync frequency is variable to change the resolution displayed on screen. The IBM PS/2 display, models 8503, 8512 and 8513 are fixed frequency monitors.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.