Panasonic KX-P1124 - Creeping Top Margin

DocumentID: 645943
Revision Date: 29-Feb-96 8:19:10 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The Panasonic KX-P1124 printer was producing a creeping top margin. The problem occurred even with a DOS print test. Solutions: The printer was set to feed the paper with the friction rollers, but the paper was loaded on the tractor feeder. Once the printer paper feed mechanism was synchronized, everything worked fine. The tractor fed paper needs to be fed below the silver bar on the printer to disable friction feed. If you feed the paper above the silver bar, the printer will beep when you try to move the lever on the left which controls friction feed/tractor feed. This problem can occur with several Panasonic printers (KX-P1124, KX- P2124, KX-P1123, KX-P2123).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.