Fax - Gateway 2000

DocumentID: 669644
Revision Date: 29-Feb-96 8:50:16 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Modem connects, but will not sent a fax. Solutions: 1. From the directory where the fax files are installed (C:\WP60; C:\WP61; C:\WP51 by default), type Setup and enter the CAS Setup Utility. 2. Select 2. Hardware Driver Setup. 3. Go to the Optional Parameters line. 4. Type in /TYPE=107. 5. Press F10 until back at DOS. 6. Reboot or unload and reload FAXDIR. The /TYPE=107 switch may or may not work. Causes: The Gateway 2000 machines use a USR Sportster modem manufactured by US Robotics. The Sportster has significant problems both sending and receiving faxes using FAXDIR. This problem has been reported to Development.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.