Changing The Zero To A Slashed 0 On Canon Las

DocumentID: 605050
Revision Date: 29-Feb-96 1:30:44 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Problem: A customer wanted the number 0 (zero) slashed instead of unslashed. Canon Laser printers can accomplish this through an initialization string. The steps to change to a slashed 0 are as follows: 1. Retrieve the .PRS or .ALL file into the PTR Program and press Enter on the printer name 2. Press Enter on Initialize and Reset 3. Press the down arrow to Initialize at Start of Print Job, press the right arrow or Ctrl-Enter 4. At the end of the string add [27,91,75,3,0,0,37,2] 5. Exit and save the file 6. If you made changes to the .ALL file, update the .PRS file in WP by pressing Print (Shift-F7), S (Select Printer), 7 (Update). NOTE: WPCorp does not support these changes. The operator should enter an enhancement request for the customer so WPCorp can keep track of how many people would really like this change. The operator that helps the customer with these changes is responsible for supporting the changes in the printer driver. An STR should NOT be written if there is a problem with this, as it is not supported. Please see memo EDT_255 for more information on this.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.