IBM 4019 LaserPrinter E (PostScript) - Changi

DocumentID: 646373
Revision Date: 29-Feb-96 8:19:14 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer requested that the redline gray shade be darker on the IBM 4019 LaserPrinter E (PostScript). This can be changed by editing the prologue variable in the PTR Program. There are three procedures, _red, _rshow, and _redshow, that need to be modified. Currently the driver asks for .95 setgray. If a customer wants a darker shade, they would need to change the value to less than .95. (ex. .75) *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.