Microsoft Lan Manager Until Supported, Use /N

DocumentID: 652639
Revision Date: 29-Feb-96 8:29:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer would like to have Microsoft Lan Manager as a supported network. His /PS and /NT options are being ignored. Solutions: Due to testing on the Lan Manager 2.0, the /NT-4 (or /NT=4) is the correct selection. This is the selection to be used until the network is formally supported. This network is basically the same as the MS LAN Manager.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.