Digital Letter Printer 100 - Suggested Emulat

DocumentID: 646853
Revision Date: 29-Feb-96 8:19:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Although the Digital Letter Printer 100 is not currently supported, one customer was able to get this printer to work in WordPerfect by selecting the Standard Typewriter definition and by making the following settings: Serial settings: 1200, ODD Parity, 7 Data Length, 1 Stop Bit, XON\XOFF - Off Dip switch settings: SW1: 1,2,3,5,8 on 4,6,7 off SW2: 1,3,5,6,8 on 2,4,7 off This printer is a daisywheel printer and the dip switches are located inside the printer underneath the print head path. This printer is not the same as the Digital LA 100.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.