NEC Silentwriter LC-890 Not Pulling From Bin

DocumentID: 634161
Revision Date: 29-Feb-96 3:03:34 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: If all efforts fail at getting the LC-890 to pull from the top/front tray (bin 2), have the customer pull out the coiled grey power cord that is connected to the bin and then plug it back in firmly. Without a proper connection the bin will never react. The connection seems to come loose over time. Some customers have gone for years without being able to print from bin 2, and this simple fix takes care of it. Physical description The LC-890 has two trays at the back of the printer. Bin #1 is the back bin when looking at the printer from the front. Bin #2 is the front bin and it sits higher than bin 1. The top one is often referred to as the front tray; it is not, however, on the front of the printer. A gray cord, like a telephone cord, comes out of the back of the printer and connects to the left side of the top tray. Though the connection may appear to be complete, it may need to be pushed in further.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.