LaserMaster Printers - Doing Duplex With Odd

DocumentID: 602256
Revision Date: 29-Feb-96 1:29:30 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The last page does not eject from the printer when using a LaserMaster printer, duplex, and an odd number of pages. Solutions: This problem will only occur with LaserMaster. They have no way of sending a Reset string to the printer at the end of the job. If this were possible they would not have a problem. WP does not send an extra form feed for odd pages when duplexing. The reason why the HP duplex printers do not have any problem is because they reset the printer at the end of the job, which causes the page ejection. A workaround is to add an extra page break to the end of the document. Status: Sent to Development ***|sent to dev|*** Press Enter on link token.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.