Star NB24-10/NB24-15 - Dip Switch Functions

DocumentID: 646428
Revision Date: 29-Feb-96 8:19:14 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The Star NB24-10/NB24-15 dip switch functions are as follows. All switches are set ON at the factory. This is the standard mode. Switch ON OFF 1-1 10cpi (Normal Pica) 17cpi (Condensed Pica) 1-2 Set SELECT IN signal to LOW Not fixed 1-3 Select internal characters Select optional characters 1-4 No bottom margin Set bottom margin to 1 inch 1-5 Character set #1 Character set #2 1-6 International char. set USA 1-7 International char. set USA 1-8 International char. set USA 1-9 Not used 1-10 Not used 2-1 Standard mode or IBM-P IBM-G mode or not used 2-2 Standard mode or IBM-G IBM-P mode or not used 2-3 Ignore download char. Enable download char. 2-4 Paper-out detected Paper-out not detected 2-5 Auto CR with line feed CR from host 2-6 LF from host Auto LF with CR 2-7 Print "normal zero" Print "slash zero" 2-8 1/6 inch line feed 1/8 inch line feed *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.