Different Features of the HP LaserJet IIID Pr

DocumentID: 645522
Revision Date: 29-Feb-96 8:19:07 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: 1. HP PCL 5, LaserJet family compatible. 2. Prints up to 8 pages per minute; 3.7 pages per minute in duplex mode. 3. Up to 20,000 pages per month. 4. Dual trays; duplex printing; optional envelope feeder. 5. The dual trays are interchangeable with other HP;s. 6. The envelope feeder is not interchangeable - holds 50 envelopes. 7. 300 dpi Resolution Enhancement technology. 8. 2 cartridge slots; 2 memory boards. 9. Macro cartridge support; optional Adobe PostScript. 10. 2M of memory is needed for PostScript printing. 11. One year on-site warranty. 12. Page protect feature - appears if you have 1 megabyte additional memory. When memory is reconfigured for page protection the printer erases all downloaded fonts (including permanent fonts) and all macros (including permanent macros). You must then reload any fonts and macros you need. 13. Output selector knob, located on the back panel. - nine o'clock position: turns the paper around as it feeds it through and outputs it with the print side down. - eleven o'clock position: feeds straight through and it comes out the back print side up. (Recommended for transparencies, envelopes, labels and anything that might curl). Features The Same As The HP III Printer 1. Memory - 1M; 720K available to the user. 2. Memory boards same as HP III an HP IIP. 3. Memory can be added in 1 - 2M increments up to 5M. 4. Interfaces; slot for AppleTalk. 5. 14 bitmapped fonts - 45 symbol sets. 6. 8 scalable typefaces; 35 symbol sets. sizes up to 999.75 points (over 13 inches high) 7. Capacity is 400 sheets, 20K pages per month. Additions To The Menu (LCD Screen) 1. Duplex: printer must be set in duplex mode which the 9:00 position. 2. Bind: long edge or short edge of paper (dependent on orientation). 3. To access the configuration press down on the Menu key for 4 to 5 seconds. 4. Reset 07; resets to the user defaults. 5. Reset 09 resets to the factory defaults. Error Messages 1. "Error 21" - Print Overrun - Data is too complex for the printer. Answer: reduce the page complexity to eliminate the problem or use the page protection feature. 2. "Error 56" - The output selector knob is not in the duplex position (9:00) position. Answer: Adjust the knob to the 9:00 position and press Continue. 3. "Error 56"; appears in the LCD screen if output selector knob is not set to 9 o'clock position. Use bottom try for duplexing (mandatory). Note: Always press Continue after eliminating the cause for the error message to reset the LCD screen. Control Panel Selectable Settings Menu Item Factory Range of User Selectable Set. Default Auto Cont Off Off, On I/O Parallel Parallel, Serial, Optional* Serial** RS-232 RS-232, RS-422 Baud Rate** 9600 300, 600, 24,00 4800, 9600, 19200 Robust XON** On On, Off DTR Polarity* Hi Hi, Low RET Medium Dark, Medium, Light, Off Page Protect+ Off Off, Ltr, Lgl, A4 * Appears only if an option I/O card is installed. ** Appears only if Serial I/O is selected + Appears only if optional memory is installed

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.