Panasonic KX-P1624 - Correcting Top Margin Di

DocumentID: 645332
Revision Date: 29-Feb-96 8:19:04 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer using WordPerfect printed documents with a Panasonic KX-P1624 printer. Text that was printed from DOS printed with a 13/16 top margin. Text printed from WP, with a top margin setting of 0", printed with a 15/16 top margin. A member of the Problem Resolution group suggested editing the .ALL or .PRS file in the PTR program to eliminate the difference. The editing change they suggested included inserting a specific code for the Top Printhead Bias. After making the suggested changes the differences between top margins were eliminated. Follow the steps below to make the Top Printhead Bias change: 1. Enter the PTR Program and retrieve the .PRS or the .ALL file 2. Press Enter on the Panasonic KX-P1624 driver 3. Cursor to Printer Commands and press Enter 4. Cursor to Printhead Bias (Top) and press Enter. This will move the cursor into the Expression Box. 5. Insert the code PTSIZE/4 and press Exit (F7) 6. Exit PTR saving the changes

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.