Epson EPL-7000 - SelecType Level 2 Functions

DocumentID: 646569
Revision Date: 29-Feb-96 8:19:15 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: TEST PRINT Prints two test patterns to check printer operation. CH CONFIG. Channel configuration. Sets up the operating mode, interface configuration, and the size of the printer's input buffer for each channel. MEMORY SHARE Memory Share specifies the proportion of the printers memory shared between channel S and P. CH TIMEOUT Channel Timeout. If no data is sent during the specified time period, the printer switches from one channel to the other. AUTO CONT. Automatic continue. Permits the printer to continue printing instead of stopping under certain error conditions. BEEPER Turns the beeper on or off. P-CONFIG SAVE Printer configuration save. Saves all level 2 settings as defaults so they take effect each time you turn the printer on. FACTORY RESET Returns all level 1 and level 2 settings to their factory settings. VERSION Displays the version numbers of the printers firmware components such as the controller and font. STANDBY Conserves power by reducing power to the fixing heater when the printer is not used for 30 minutes.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.