Outdenting Problem - Preferred Fix

DocumentID: 652913
Revision Date: 29-Feb-96 8:29:19 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: What is the preferred method of fixing an outdenting problem? Solutions: The preferred method to fix outdenting, would be to fix the vertical motion by forcing a carriage return with each line feed (Line Feed = [13,10], or fix the printer by changing the dip switches. Sometimes the method of vertical motion used in the driver is not VMI and cannot be set up with a carriage return for every line feed. If this is the case, and a user simply does not wish to change dip switches, a Reposition could be used. It should be placed in the relative horizontal motion so that WP will reset the horizontal position for every new line.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.