Canon BJ-10e -- Suggested Dip Switch Settings

DocumentID: 609642
Revision Date: 29-Feb-96 1:34:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: FYI: Some symptoms of incorrect dip switch settings on the Canon BJ-10e might be incorrect centering or incorrect underlining (i.e., underline appearing on wrong text.) The cause could be that dip switch 7 is down when it should be up. All 10 dip switches should be off. Switch 1 should be on if the printer has a sheet feeder attached. Turning switch 10 on will put the printer in IBM mode.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.