Print - Serial Printing At 19,200 Baud Rate

DocumentID: 646437
Revision Date: 29-Feb-96 8:19:15 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: A customer was using a DOS Utility that allowed him to print serially at 19,200 baud rate. Using the utility, he was able to print from DOS at that speed, but when selecting that rate in WordPerfect, he was unable to get his printer to respond. Solutions: By selecting 8 for Other, then typing in LPT1 as the port (Shift-F7, S, 3, 2, 8), instead of choosing the LPT1 option from the port menu, the customer was able to print at 19,200 baud. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.