HP LaserJet III and IIID - Graphics Line Thic

DocumentID: 633918
Revision Date: 29-Feb-96 3:03:28 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: A customer wants to make a graphics line only as thick as one dot or pixel. He wants to do this on an HP LaserJet III and IIID. Solutions: Set the graphics resolution to High (Shift-F7, G, H). Then, for graphic line thickness (Alt-F9, L, H, W) use the formula /300. So if you want 1 dot thickness, you would enter in 1/300 and press Enter. For 2 dots thickness, you would enter 2/300, and so on.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.