Tandy DWP-230 - Changing Dip Switches Correct

DocumentID: 647101
Revision Date: 29-Feb-96 8:19:19 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Problem: The customer was getting garbage when printing to a Tandy DWP-230 printer. Setting the dip switches so that switch 5 was down (on) and the rest up (off) corrected the problem. This was different than the switch settings shown in PRHelp. *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.