IBM 4019 Laser Printer - Printing Envelopes

DocumentID: 645483
Revision Date: 29-Feb-96 8:19:06 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Envelopes used in the IBM 4019 Laser Printer should meet the following specifications: Length Feed Method Specification Length Auto 7.5 to 9.5 inches Manual 7.5 to 14 inches Width Auto 3.875 to 6.9 inches Manual 3.625 to 8.5 inches Weight Auto 20 to 24 lbs. Manual 20 to 28 lbs. When manually feeding envelopes, always wait for the Check, Envelope and Manual lights to come on, and a 3 to be displayed before placing an envelope in the manual feed tray. Placing an envelope in the tray prior to this could cause unexpected results. If the printer is operating in HP Emulation mode change the print orientation to Landscape. When placing envelopes in the envelope feeder, the feeder shows to place the stamp corner of the envelope to the bottom right of the feeder. The manual on the other hand, shows to place the stamped corner in the upper left of the feeder. The printer manual diagram is correct, and the diagram on the printer itself appears to be wrong.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.