Citizen 200GX - Accessing The Dip Switches

DocumentID: 606483
Revision Date: 29-Feb-96 1:31:43 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The Citizen 200GX dip switches are located under a serial interface. The user will need to use their thumb to remove the serial interface. The switches are found directly under the removed part. This interface is on the right side of the printer above the printer port.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.