Epson ActionLaser II - How To Check The Mode

DocumentID: 641570
Revision Date: 29-Feb-96 8:18:38 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: To see what the mode setting is on the Epson ActionLaser II printer, hold down the SELECTYPE button until it says SELECTYPE LEVEL 2 (the printer will automatically go off-line). It will say this briefly. Then press the Down Arrow (under the Manual button) until it says MODE ASSIGN. Then press the Right arrow (under the on-line button) and a code will appear that looks like P HP LJ-2P. The first letter stands for either P (Parallel), S (Serial), or O (optional if an optional interface is installed). Use the Up or Down arrows to choose the interface you want, then press the right arrow. An arrow will point at the current printer (either HP LJ-2P, Epson FX, or Epson LQ). Use the Up or Down arrow to choose the printer you want then press the Right arrow to confirm it. To exit, press the SELECTYPE button (Left arrow) until the printer comes back on line.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.