Foot-Lambert Definition

DocumentID: 656321
Revision Date: 29-Feb-96 8:29:42 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Foot-Lambert: One foot-lambert equals 1 divided by pi candela per square foot. A foot-lambert (FL) is the unit for measuring the screen luminance of the video display. A candela is the modern measure of luminous intensity, roughly equal to the light given off by a candle.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.