Hayes Optima 96/24 Fax/Modem - How To Receive

DocumentID: 632609
Revision Date: 29-Feb-96 3:03:02 PM

The information in this document applies to:
WordPerfect® 6.1 for DOS

Problem

Using WordPerfect's FAXDIR.EXE with a Hayes Optima 96/24 Fax/Modem results in the modem not being able to receive faxes.

Answer:

Run the CAS setup utility and place /ANS=1 on the optional parameters line.

Details:

When the string /ANS=1 is placed in the optional parameters of the Setup utility, and if the Class 2 driver is used, the modem will receive faxes.

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.