Envelopes - Wrinkling When Printing

DocumentID: 600459
Revision Date: 29-Feb-96 1:28:25 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: If a customer finds that their envelope wrinkles each time they print on a laser printer, try having them put the envelope in a microwave for 15-30 seconds. This will not damage the seal of the envelope and has been successful for some customers. Please make sure the envelopes aren't embossed or lined with any metallic materials.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.