PostScript Printers And The Three Types Of Ti

DocumentID: 626425
Revision Date: 29-Feb-96 1:41:36 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: PostScript printers generally have three types of timeouts: 1. Job timeout - This is the amount of time allowed for the print job to complete. 2. Manual timeout - This is the amount of time that the printer will wait for you to put the paper in the printer on a manual feed job. 3. Wait timeout - This is the amount of time that it will wait, after the buffer is full on the printer, to receive more data from the computer. These three timeouts are set with the TIMOUTS.PS file. They are represented in the line 0 60 0 setdefaulttimeouts. In the previous example, the first 0 is the job timeout, the 60 is the manual timeout value, and the last 0 is the wait timeout. (The value of 0 is infinite, any other value is time in seconds.)

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.