Tandy DMP 2100 - Correcting Outdenting

DocumentID: 646942
Revision Date: 29-Feb-96 8:19:18 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The following steps may be used to correct random outdenting that may occur on the Tandy DMP 2100 printer: 1. Enter the PTR Program and retrieve the .PRS file 2. Press Enter on Vertical Motion 3. Press Enter on Relative Vertical Motion 4. Highlight Move Down and press Right Arrow to enter the Expression box 5. Press Ctrl-Enter to move the expression to the lower box 6. Press Home, Home, Down Arrow 7. Type "REPOSITION" and press F7 8. Save the file and exit the PTR Program

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.