TI MicroLaser (PostScript) Release Notes Vers

DocumentID: 647323
Revision Date: 29-Feb-96 8:19:20 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The information below is for the TI microLaser (Postscript) printer version 1.3. 1. Some of the serial COMM errors will cause the printer to lock up with the COMM error message displayed on the printer's LCD. These errors will require the user to turn power off, then on before the COMM parameters or error condition can be corrected. COMM errors that deal with incorrect baud rates, parity, and buffer overflow will cause this problem. 2. If an error condition (i.e. opening the top cover, removing the paper tray, etc.)occurs during power up of the printer and before the "Online/Offline" LED is on, then the printer's control panel may not function properly. To fix this problem, correct the error condition and turn the printer off, then back on.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.