Editing The DOS Text Printer To Eliminate Lon

DocumentID: 628387
Revision Date: 29-Feb-96 1:42:27 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer wants to use the DOS Text printer definition to create ASCII files to transmit through Microsoft e-mail. To do this the lone carriage returns ([13]) need to be eliminated. Solutions: The customer can edit the DOS Text printer driver using the following steps: 1. Using the PTR Program, retrieve the .PRS file 2. Press Enter on DOS Text Printer 3. Press Enter on Horizontal Motion 4. Press Enter on Relative Horizontal Spacing (microspace) 5. Cursor to the right of Perform Carriage Return 6. Change the [13] to [13,10] 7. Cursor to the right of Auto Line Feed on Carriage Return? 8. Change it from NO to YES 9. Exit and save the .PRS file.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.