Quadram JT FAX - Selecting A Port

DocumentID: 634486
Revision Date: 29-Feb-96 3:03:42 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: What port should be selected when using the Quadram JT FAX board? Solutions: Customers should select the LPT1 port after selecting the application capture in the JT FAX software program.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.