IBM Quietwriter III - Setting Dip Switch 4 To

DocumentID: 646368
Revision Date: 29-Feb-96 8:19:14 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: When printing to the IBM Quietwriter III, if dip switch 4 is on, the printer may beep and go off-line. Users should then press the On-line button to continue the print job. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.