LaserMaster LX6 - Unable To Duplex With HP La

DocumentID: 645321
Revision Date: 29-Feb-96 8:19:04 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The user cannot print duplex with the LaserMaster LX6 driver. They can print simplex and duplex fine with the HP LaserJet IID selected. When trying to print duplex, WordPerfect says it is printing and sends the job, but the job never prints. Solutions: If you have the LaserMaster LX6 (800 dpi) board, you must use the 600 dpi driver and have a minimum of 6M of memory on the board. If you have the 600 dpi board and wish to duplex using the 600 dpi driver, you also need a minimum of 6M of memory on the board, if you do not you must use the 300 dpi driver. Even though WP will tell LaserMaster to duplex, if LM finds there is not enough memory to place both imaged pages on the board to duplex, it will switch to simplex. When duplexing was tested with the 600 dpi driver and only 4M of memory on the LM board, the printer didn't duplex. When retested with the 300 dpi driver, it worked perfectly.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.