IBM Quietwriter - Printing Dip Switch Setting

DocumentID: 628861
Revision Date: 29-Feb-96 1:42:34 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer can print the current dip switch settings on the IBM Quietwriter printer by pressing the STOP button while turning on the printer. The dip switch settings will usually be proceeded by an M (M001100). If a user receives an H (H001100) or an L (L001100), it's fine. The letter refers to the contrast control on the printer, i.e., Low, Medium, and High.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.