QMS Kiss or QMS Kiss Plus (Module 20/30) Prin

DocumentID: 647263
Revision Date: 29-Feb-96 8:19:20 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The customer had a QMS Kiss printer connected through a switchbox. He kept getting a blank page after every print job. He also had 5.0 on this same computer and was not getting a blank page. We matched up the codes from his 5.0 .PRS file to his 5.1 .PRS file. Someone had modified the 5.0 file--when we made the same change to the 5.1 file, an extra page no longer came out on the printer. What we did was: 1. Go into PTR 5.1. 2. Retrieve WPLA1.ALL or QMSKISS.PRS. 3. Go to "Initialize and Reset" and Enter. 4. Go to "Reset at End of Print Job" and Enter. This currently reads [27]"[99r". Change it to read [27]"c"[12]. 5. Save and exit. Update if the change was made to the .ALL file.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.