Juki 6300 - Paper Should Be Loaded Over The T

DocumentID: 646340
Revision Date: 29-Feb-96 8:19:14 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Customers using the Juki 6300 printer should load their continuous paper over the top of the paper tension bar. This bar is found on the track feeder and can be identified by a black lever on the right side of the printer. One customer who did not have their paper set in this way would only get the first page of a document to print. A red, alert light would then go on. Changing the location of the paper corrected their problem. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.