NEC Spinwriter 7710, NEC Spinwriter 8810 Prin

DocumentID: 645683
Revision Date: 29-Feb-96 8:19:08 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using two unsupported printers. One is the NEC Spinwriter 7710 and the other is the NEC Spinwriter 8810. The users have selected NEC Spinwriter 3510 which is the suggested emulation for both printers. When using underline, the printers print too far to the right of the underlined character as compared to other lines in the document. The underlined spaces seem to be cutting short by about a half a space. The print wheel being used is the New Prestige Elite Legal A. The document looks correct in View Document, but when it prints the underline cuts slightly short. Solutions: A tab code was not being used on the lines where the underline was not lining up with the other underlined numbers above and below. Part of the problem also is contributed to the fact that the printer does not have an auto underline command. Therefore, WordPerfect has to do the underline on a separate pass. In addition, there is a -25 in the adjust for the underline command in the PTR program which prevents the underline character [95] from showing gaps. Taking out this adjustment seems to help. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.