NEC Spinwriter 8850 (8800) Using the NEC 4523

DocumentID: 647669
Revision Date: 29-Feb-96 8:19:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: When purchasing the NEC Pinwriter P5 or the NEC Spinwriter 8850 (8800) the NEC 4523 single bin Cut Sheet Feeder normally sells with it. When using this sheet feeder with the NEC 8850 one may want to select the NEC 3550 Single/Dual SF sheetfeeder and set the location to Bin 1. When the printer is defined the default sheet feeder selection is NONE and the form location is Continuous. When using these settings the customer may experience problems with the paper not pulling from the bin. Changing the sheet feeder and forms location to what was mentioned above has been found to correct the problem.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.