Canon BJ-130e - Courier 12cpi Not 6 Lines Per

DocumentID: 616801
Revision Date: 29-Feb-96 1:37:29 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using the Canon BJ-130e printer. When selecting a Courier 12cpi font, the line height adjusts to 5.15 lines per inch (LPI) instead of 6 LPI. After selecting the Gothic 12cpi font, the line height remains at 6 LPI. Solutions: This problem will not be addressed in WP 5.1 due to document portability. This problem may be addressed in a future version of WordPerfect. The customer can make the following changes in the printer driver to get 6 LPI with the Courier 12cpi font selected: 1. Enter the PTR Program, retrieve the WPMS1.ALL file, select the Canon BJ-130e printer, and press Enter 2. Move to Fonts and press Enter twice 3. Move to the Courier 12cpi font and press Enter 4. Move to Size and Spacing and press Enter 5. Move to Leading Adjust and press the right Arrow key once 6. Delete the 2 7. Press F7 until you are prompted to save the file. Save the file and exit the PTR Program. 8. Update the .PRS file in WordPerfect (Shift-F7, S, 7)

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.