Manual Feed And Envelope Feeder On IBM LaserP

DocumentID: 641491
Revision Date: 29-Feb-96 8:18:37 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The manual feeder and the envelope feeder on the IBM 4019 and 4029 LaserPrinters are the same part. The sheet feeder does not have a setting for manual paper, so customers should leave the location at manual even though they have a sheet feeder selected. The manual feed slot is not the same as the envelope feed slot. The manual feed goes above the envelopes at a slight angle with a curved piece between it and the envelope feed slot. The printer will come up with a 3 for manual feed, and when the customer presses the Print/Check button, the number that corresponds with the paper that the printer is expecting to print on will display. If the printer recognizes the paper, it will pull the paper through. There is no other button like a form feed button. If the printer says something like 2 but does not pull the paper through, the customer can try re-adjusting the paper and make sure it is in the correct location (not in the envelope tray which can confuse customers). *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.