8514/A Definition

DocumentID: 655536
Revision Date: 29-Feb-96 8:29:37 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: 8514/A: The 8514/A is an advanced, high-resolution analog video display adapter from IBM originally designed for the PS/2 line of personal computers. Compared to previous display adapters such as EGA and VGA, it provides a high resolution of 1024x768 pixels with up to 256 colors or 64 shades of gray. It is an interlaced display which means that it scans every other line each time the screen is refreshed. It provides a video co-processor that performs two dimensional graphics functions internally, thus relieving the CPU of graphics tasks. The 8514/A monitor improves the performance of CAD applications by as much as ten times.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.