NEC Spinwriter 3510 Not Printing Bold

DocumentID: 645005
Revision Date: 29-Feb-96 8:19:02 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer cannot get Bold on the NEC Spinwriter 3510. Solutions: Please watch SCNs to see this change after the 08/20/90 printer.ALL file release. As a temporary fix the customer can do the following steps in the PTR Program: 1. Retrieve the .ALL file 2. Press Enter on the NEC Spinwriter 3510 printer 3. Press Enter on Attribute Methods 4. Press Enter on Bold 5. Mark Triple Overstrike on the Same Pass with an asterisk (*) 6. Press Enter twice 7. Set the Offset to 3 8. Exit and save the file. Then update the .PRS file in WP (Shift-F7, S, 7).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.