MoreFonts RUN WPS Warning Not Printing On HP

DocumentID: 600296
Revision Date: 29-Feb-96 1:28:22 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: If the user does not use the command WPS to start MoreFonts and enter WP, the words RUN WPS will appear on the printout if they try to print a document using a MoreFonts soft font. The RUN WPS warning no longer prints out when using MoreFonts and the HP LaserJet III printer release later than 04/12/90. Solutions: After the 04/12/90 printer release, a modification was made to the printer driver to set the image area of the page. Prior to sending the command to set the area, a zero (0) Y positioning code is sent. The Y positioning code is sent at the end of the Set Page Length string in the HP LaserJet III type printer drivers. The warning RUN WPS is still being sent, but the printer is not printing it because the text is printing in the unprintable zone. The customer should not remove the zero Y positioning code because it is sent prior to the area imaging code. This is not a MoreFonts problem or a WPCorp problem. It is simply a load string not printing because the printer is started at position zero (0). The customer will just need to make sure that they use the WPS command to enter WP.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.