QMS ImageServer X320 Printer - General Inform

DocumentID: 646787
Revision Date: 29-Feb-96 8:19:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The QMS ImageServer X320 printer supports PostScript and imPRESS page description languages. The following emulations are resident: HP PCL, HP- GL, Diablo 630 ECS, Epson-FX+, IBM 5152, Tektronix 4010/4014, and IBM 1403. This printer features three multibus 68000-class processors (including the 68020) which work together to free host systems from intensive print management tasks, thereby increasing productivity. This printer also uses Real-Time Rasterization, a proprietary process that allows page compilation and printing to occur simultaneously using a 2.5M raster image buffer. The QMS ImageServer X320 has a rated print speed of 20 pages per minute, and includes a broad range of interface support. It provides advanced paper handling capabilities such as electronic page collation, page order reversal, transparent jam recovery, and multiple collated copies. It also supports 11" x 17"/A3 paper sizes.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.