IBM Quietwriter I (Old EPROM) - Second Print

DocumentID: 645631
Revision Date: 29-Feb-96 8:19:08 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using an IBM Quietwriter I (Old EPROM) printer. The printer prints the first print job fine. The second print job usually prints 3-4 lines, ejects a blank page, prints 3-4 lines, and then repeats. If the customer turns off the printer between print jobs, everything works fine. The customer has a sheet feeder but none is selected. And his forms are set to continuous. His printer works fine in other applications and from DOS. Solutions: This is fixed with a new Eprom.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.