Computer Locks When Stacking Print Jobs (.PCX

DocumentID: 615083
Revision Date: 29-Feb-96 1:36:39 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: A customer's computer was locking when stacking print jobs containing .PCX graphics files. The customer was using Stacker 3.0. Solutions: The customer reversed the position of the two IDE hard drives so that the master drive was at the end of the cable and the slave was in the middle. After doing this the problem disappeared.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.