HP LaserJet - Accessing A Line Printer 16.67c

DocumentID: 645930
Revision Date: 29-Feb-96 8:19:10 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The HP LaserJet printer does not have an internal 16.67cpi font. Because of this, printer command strings cannot be used to access a Line Printer 16.67cpi font. One customer was using a custom made cartridge that contained this font. In order to access the font, they entered the PTR program and marked the HP LaserJet Series II - Line Printer 16.67cpi font as being built-in. After marking the font, the user updated the .PRS file in WordPerfect. The following is the list of steps taken by the user: 1. Enter the PTR program 2. Retrieve the WPHP1.ALL file 3. Press Enter on HP LaserJet 4. Press Enter on Fonts 5. Cursor to the HP LaserJet Series II font listed under Built-In and press Enter 6. Mark the Line Printer 16.67cpi font with an asterisk 7. Press F7 8. Mark the HP LaserJet Series II font with an asterisk 9. Exit the PTR program, saving the changes 10. Update the .PRS file in WordPerfect (Shift-F7, S, U) Customers who do not have a cartridge containing the Line Printer 16.67cpi font may have another option. Some users have obtained this font by simply selecting the HP LaserJet Series II driver. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.