Print to Hardware Port Changed To Increase Pr

DocumentID: 652079
Revision Date: 29-Feb-96 8:29:13 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using the HP LaserJet III printer which is printing extremely slow. It took a minute and a half to print the phrase "this is a test" with a Courier 12pt font selected. Solutions: The problem is solved by changing the printer's Print to Hardware Port to Yes (Shift-F7, S, E, 7). This is not WordPerfect's preparation of the print job, but a hardware problem. Changing the Print to Hardware Port to Yes, by-passes the print bios allowing WP to handle the output of the print job rather than the computer.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.