Toshiba P1340 Character 4,34 "Em Dash"

DocumentID: 647665
Revision Date: 29-Feb-96 8:19:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The "em dash", character 4,34 is not printing correctly on the Toshiba P1340 printer. The character is printing too low on the line of text. It views correctly. Solutions: The 4,34 character is not mapped in this printer driver and is therefore printing graphically. To print the character higher the customer could change the graphic bias or print the ASCII dash. To make it much simpler, the customer could print character 3,8 (also a dash) using any of the following fonts: P1350 Built In, P321 (IBM), P321, P341e, SL Built In or SL (SA).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.