QMS PS 810 Problem - Expanded Memory, Flush R

DocumentID: 644804
Revision Date: 29-Feb-96 8:19:01 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using the QMS PS 810 printer. In tables using cell features flush right and small caps together, the text will print over the right line of the cell. The customer turned off his 386 To The Max program and everything worked fine. Using the /NE startup switch without turning off 386 To The Max also worked. Creating the table and then assigning the attributes using Ctrl-F8 works fine in either case. Solutions: The 386 To The Max program takes extended memory and causes it to emulate expanded memory. WPCorp has seen several problems in this situation because of a technique WP uses called "data aliasing". WP used this technique on the original WP 5.1 release, but found that it causes problems with many of these expanded memory emulators. Future releases of WP 5.1 will not use data aliasing. In the meantime, the customer can work around the problem by using the /NE startup option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.